11/8/94

MIPS R4000 Microprocessor User’s Manual Errata for the 2nd. Edition, 1994

This document contains information that is proprietary to MIPS Technologies, Inc. MIPS Technologies, Inc. reserves the right to change any products described herein to improve the function or design. MIPS Technolgies, Inc. does not assume any liability arising out of the application or use of any product or circuit described herein; neither does is convey any license under patent rights nor imply the rights of others.

Copyright 1994 by MIPS Technologies, Inc. All rights reserved.

MIPS Technologies Inc. 2011 N Shoreline Blvd PO Box 7311 Mountain View, CA 94039-7311

Errata for MIPS R4000/R4400 Micr oprocessor User’s Manual, 2nd. Edition

November 8, 1994

This errata supplements the "MIPS R4000/R4400 User’s Manual, 2nd Edition" by Joe Heinrich

11/8/94

MIPS R4000 Microprocessor User’s Manual Errata for the 2nd. Edition, 1994

This document contains information that is proprietary to MIPS Technologies, Inc.

MIPS Technologies, Inc. reserves the right to change any products described herein to improve the function or design. MIPS Technolgies, Inc. does not assume any liability arising out of the application or use of any product or circuit described herein; neither does is convey any license under patent rights nor imply the rights of others.

Copyright 1994 by MIPS Technologies, Inc. All rights reserved.

MIPS Technologies Inc.

2011 N Shoreline Blvd

PO Box 7311

Mountain View, CA 94039-7311

Errata for MIPS R4000/R4400 Micr oprocessor

User’s Manual, 2nd. Edition

November 8, 1994

This errata supplements the "MIPS R4000/R4400 User’s Manual, 2nd Edition" by Joe Heinrich

Page 229

At the end of the section titled SyncIn/SyncOut, add the following:

The delay allowed between the SyncOut and SyncIn must be no more than [1/2*MasterClock cycle - 2nS]

Page 319

In Table 12-3, for Page Attribute "Exclusive" the Processor Configuration should be only R4000MC (remove "R4000SC)

Page 338

At the end of the sentence in the ninth line: "Figures 12-24 through 12-27 illustrate ....... below. Add the following sentence: "All the waveforms are shown with zero delay from the SClock’s rising edge; i.e. outputs are driven by the processor at the corresponding rising edge and inputs are driven by the external logic at the corresponding rising edge of the SClock.

Also at the end of the paragraph describing Figure 12-24: "Figure 12-24 illustrates .... WrRdy*. Add the following sentence: "In this example, the WrRdy* must be deasserted in cycle 5 (sampled by the processor at the rising edge of cycle 6) to delay the issue cycle that would have occurred in cycle 7. Assertion of WrRdy* in cycle 8 (sampled by the processor at the rising edge of cycle 9) will cause the Write Request to be issued in cycle 10.